{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","40","42","44","45"]
["","","","Средн.","дБA","34","38","40","41"]
["","","","Тихая работа","дБA","21","30","32","33"]
["","","","Низк.","дБA","28","33","35","36"]
["","Охлаждение","","Средн.","дБA","33","39","41","42"]
["","","","Тихая работа","дБA","20","31","33","34"]
["","","","Низк.","дБA","26","34","36","37"]
["","","","Выс.","дБA","40","43","45","46"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1","1","1"]
["","Руководство по эксплуатации","","","","1","1","1","1"]
["","Пульт дистанционного управления","","","","1","1","1","1"]
["","Сухие батареи AAA","","","","2","2","2","2"]
["","Держатель пульта дистанционного управления","","","","1","1","1","1"]
["","Монтажная пластина","","","","1","1","1","1"]
["","Крепежные винты внутреннего блока","","","","2","2","2","2"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.50","12.7","12.7","12.7"]
["","Дренаж","","","","18","18","18","18"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.019","0.029","0.032","0.032"]
["","Hагрев","","Ном.","кВт","0.020","0.032","0.035","0.035"]
["Уровень звуковой мощности","Охлаждение","","","дБA","55","59","60","62"]
["","Отопление","","","дБA","55","61","62","62"]
["Размеры","Блок","","Ширина","мм","770","990","990","990"]
["","","","Глубина","мм","225","263","263","263"]
["","","","Высота","мм","286","295","295","295"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый"]
["Масса","Блок","","","кг","8.50","13.5","13.5","13.5"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","10.3","17.3","17.9","17.9"]
["","","","Низк.","м³/мин","6.7","12.2","12.8","12.8"]
["","","","Средн.","м³/мин","8.6","14.8","15.8","15.8"]
["","","","Тихая работа","м³/мин","5.3","10.7","11.3","11.3"]
["","","Охлаждение","Низк.","м³/мин","6.1","11.9","12.2","12.2"]
["","","","Средн.","м³/мин","8.1","14.4","14.8","14.8"]
["","","","Выс.","м³/мин","10.1","16.8","17.3","17.3"]
["","","","Тихая работа","м³/мин","4.4","10.5","10.7","10.7"]
["Power supply","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Наименование","","","","","V1","V1","V1"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240"]
["Входная мощность","Охлаждение","","Ном.","кВт","","","","","0.019","0.032"]
["","Hагрев","","Ном.","кВт","","","","","0.02","0.032"]
["Корпус","Цвет","","","","","","","","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","","","","286","286"]
["","","","Ширина","мм","","","","","770","770"]
["","","","Глубина","мм","","","","","225","225"]
["Масса","Блок","","","кг","","","","","8.5","9"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","","","","10.1","11.5"]
["","","","Средн.","м³/мин","","","","","8.1","8.3"]
["","","","Низк.","м³/мин","","","","","6.1","6.3"]
["","","","Тихая работа","м³/мин","","","","","4.4","4.5"]
["","","Hагрев","Выс.","м³/мин","","","","","10.3","11.5"]
["","","Нагрев","Средн.","м³/мин","","","","","8.6","9"]
["","","Hагрев","Низк.","м³/мин","","","","","6.7","7"]
["","","","Тихая работа","м³/мин","","","","","5.3","5.3"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","","","","55","58"]
["","Отопление","","","дБA","","","","","55","58"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","","","","","40","43"]
["","","","Средн.","дБA","","","","","33","34"]
["","","","Низк.","дБA","","","","","26","27"]
["","","","Тихая работа","дБA","","","","","20","20"]
["","Hагрев","","Выс.","дБA","","","","","40","40"]
["","Нагрев","","Средн.","дБA","","","","","34","35"]
["","Hагрев","","Низк.","дБA","","","","","28","29"]
["","","","Тихая работа","дБA","","","","","21","21"]
["Подсоединение труб","Жидкость","","НД","мм","","","","","6.35","6.35"]
["","Газ","","НД","мм","","","","","9.5","9.5"]
["","Дренаж","","","","","","","","18","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","","","","","ARC470A1","ARC470A1"]
["","Проводной пульт дистанционного управления","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Электропитание","Фаза","","","","","","","","1~","1~"]
["","Частота","","","Гц","","","","","50","50"]
["","Электропитание-=-Напряжение-=-В","","","В","","","","","220-240","220-240"]