{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":12,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B"]
[]
[]
[]
[]
["","","","","","FCAG35BVEB","FCAG50BVEB","FCAG60BVEB","FCAG71BVEB","FCAG100BVEB","FCAG125BVEB","FCAG140BVEB"]
["Холодопроизводительность","Общая производительность","","Ном.","кВт","3.50","5.00","5.70","6.80","9.5","12.1","13.40"]
["Теплопроизводительность","Общая производительность","","Ном.","кВт","4.2","6.0","7.0","7.5","10.8","13.5","15.5"]
["Корпус","Материал","","","","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","204","204","204","204","","","246"]
["","","","Ширина","мм","840","840","840","840","840","840","840"]
["","","","Глубина","мм","840","840","840","840","840","840","840"]
["Масса","Блок","","","кг","18","19","19","21","23","23","23"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","12.9","14.6","14.9","15.1","22.7","27.2","27.2"]
["","","","Средн.","м³/мин","10.6","11.8","12.2","13","17.8","20.4","20.4"]
["","","","Низк.","м³/мин","8.8","9.4","9.6","10.8","13","13.1","13.1"]
["","","Hагрев","Выс.","м³/мин","14.1","14.6","14.9","15.1","23","27","27"]
["","","Нагрев","Средн.","м³/мин","11.6","11.8","12.2","12.9","18.1","20.2","20.2"]
["","","Hагрев","Низк.","м³/мин","9.4","9.4","9.6","10.8","13.2","13","13"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","49","49","51","51","54","58","58"]
["","Отопление","","","дБ(A)","49","49","51","51","54","58","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","31","31","33","35","","","41"]
["","","","Средн.","дБ(A)","29","29","31","31","33","35","35"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","27","27","28","28","","","29"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","31","31","33","33","","","41"]
["","Нагрев","","Средн.","дБ(A)","29","29","31","31","33","35","35"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","27","27","28","28","","","29"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Газ","","НД","мм","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Дренаж","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Декоративна панель","Модель","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Размеры","","Высота","мм","65","65","65","65","65","65","65"]
["","","","Ширина","мм","950","950","950","950","950","950","950"]
["","","","Глубина","мм","950","950","950","950","950","950","950"]
["","Масса","","","кг","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["Декоративная панель 2","Модель","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Размеры","","Высота","мм","148","148","148","148","148","148","148"]
["","","","Ширина","мм","950","950","950","950","950","950","950"]
["","","","Глубина","мм","950","950","950","950","950","950","950"]
["","Масса","","","кг","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["Декоративная панель 3","Модель","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Размеры","","Высота","мм","106","106","106","106","106","106","106"]
["","","","Ширина","мм","950","950","950","950","950","950","950"]
["","","","Глубина","мм","950","950","950","950","950","950","950"]
["","Масса","","","кг","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["Системы управления","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Электропитание-=-Частота","","Частота","","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Электропитание-=-Напряжение","","Напряжение","","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Размеры","Блок","","Высота","мм","","","","","246","246"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","","","","","37","41"]
["","","","Низк.","дБA","","","","","29","29"]
["","Hагрев","","Выс.","дБA","","","","","37","41"]
["","","","Низк.","дБA","","","","","29","29"]
["Системы управления","Инфракрасный пульт ДУ","","","","","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]