{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Уровень звукового давления","Hагрев","Выс.","дБ(A)","35","35","38","38"]
["","","Средн.","дБ(A)","33","33","35","35"]
["","","Низк.","дБ(A)","27","27","30","30"]
["","Охлаждение","Средн.","дБ(A)","33","33","35","35"]
["","","Низк.","дБ(A)","27","27","30","30"]
["","","Выс.","дБ(A)","35","35","38","38"]
["Стандартные аксессуары","Инструкции по установке","","","1","1","1","1"]
["","Руководство по эксплуатации","","","1","1","1","1"]
["","Изоляция фитинга","","","1","1","1","1"]
["","Уплотнительная подушка","","","1","1","1","1"]
["","Металлический зажим","","","1","1","1","1"]
["","Сливной шланг","","","1","1","1","1"]
["","Шайба для подвесного кронштейна","","","8","8","8","8"]
["","Уплотнительный материал","","","2","2","2","2"]
["","Зажимы","","","6","6","6","6"]
["","Крепежная пластина шайбы","","","4","4","4","4"]
["","Винты для фланцев воздуховодов","","","1","1","1","1"]
["","Воздушный фильтр","","","1","1","1","1"]
["Подсоединение труб","Жидкость","НД","мм","6.35","6.35","6.35","6.35"]
["","Газ","НД","мм","9.50","9.50","12.70","12.70"]
["","Дренаж","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Входная мощность","Охлаждение","Ном.","кВт","0.036","0.036","0.060","0.060"]
["","Hагрев","Ном.","кВт","0.036","0.036","0.060","0.060"]
["Уровень звуковой мощности","Охлаждение","","дБ(A)","53","53","55","56"]
["","Отопление","","дБ(A)","53","53","55","56"]
["Размеры","Блок","Ширина","мм","750","750","1,150","1,150"]
["","","Глубина","мм","620","620","620","620"]
["","","Высота","мм","200","200","200","200"]
["Масса","Блок","","кг","21","21","28","28"]
["Вентилятор","Внешнее статическое давление","Ном.","Па","30","30","40","40"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Частота","","Гц","50","50","50","50"]
["","Напряжение","","V","220-240","220-240","220-240","220-240"]