{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B (Archived)","FTXTM40M2V1B (Archived)"]
["Входная мощность","Охлаждение","","Ном.","kW","0.032","0.037"]
["","Hагрев","","Ном.","kW","0.037","0.04"]
["Корпус","Цвет","","","","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","294","300"]
["","","","Ширина","мм","811","1040"]
["","","","Глубина","мм","272","295"]
["Масса","Блок","","","кг","10","14.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","11.7","15.5"]
["","","","Средн.","м³/мин","8","9.2"]
["","","","Низк.","м³/мин","6.3","5.7"]
["","","","Тихая работа","м³/мин","5.2","4.6"]
["","","Hагрев","Выс.","м³/мин","12.2","17.7"]
["","","Нагрев","Средн.","м³/мин","7.5","11"]
["","","Hагрев","Низк.","м³/мин","5.1","7.5"]
["","","","Тихая работа","м³/мин","4.1","6.3"]
["Уровень звуковой мощности","Охлаждение","","","дБA","60","60"]
["","Отопление","","","дБA","61","61"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","45","46"]
["","","","Средн.","дБA","33","32"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","24"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","21","20"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","45","46"]
["","Нагрев","","Средн.","дБA","31","31"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","22","22"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","19","19"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5"]
["","Дренаж","","","","16 (внутренний диаметр соединительного шланга)","16 (внутренний диаметр соединительного шланга)"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC466A55","ARC466A55"]
["","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Электропитание","Наименование","","","","V1","V1"]
["","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-240","220-240"]