{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N9"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B9","RXTP35N2V1B9"]
["Уровень звукового давления","Hагрев","","Ном.","дБA","49","49"]
["","Охлаждение","","Ном.","дБA","48","48"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1"]
["","Табличка с данными о заправке хладагентом","","","","1","1"]
["","Этикетки о фторированных парниковых газах на нескольких языках","","","","1","1"]
["Хладагент","Charge","","","TCO2Eq","0.75","0.75"]
["","ПГП","","","","675","675"]
["","Charge","","","кг","1.1","1.1"]
["","Тип","","","","R-32","R-32"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","450","450"]
["","","Hагрев","Самый низкий","об/мин","360","360"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Макс.","°C сух.т.","46","46"]
["","","","Мин.","°C сух.т.","-10","-10"]
["","Heating","Темп. нар. возд.","Макс.","°CWB","18","18"]
["","","","Мин.","°CWB","-25","-25"]
["Подсоединение труб","Перепад уровней","IU - OU","Макс.","м","15","15"]
["","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","763","763"]
["","","","Глубина","мм","312","312"]
["","","","Высота","мм","551","551"]
["Масса","Блок","","","кг","38","38"]
["Power supply","Phase","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-240","220-240"]
["Примечания","","","","","(1) - Содержит фторированные парниковые газы","(1) - Содержит фторированные парниковые газы"]
["","","","","","(2) - Рабочий диапазон см. в отдельных чертежах","(2) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(3) - Электрические параметры см. в отдельных чертежах","(3) - Электрические параметры см. в отдельных чертежах"]